// Copyright (C) 1999,2000 Yokogawa Electric Corporation and
//                         YDC Corporation.
// All rights reserved.
// 
// Redistribution and use of this software in source and binary
// forms, with or without modification, are permitted provided that
// the following conditions and disclaimer are agreed and accepted
// by the user:
// 
// 1. Redistributions of source code must retain the above copyright
//    notice, this list of conditions and the following disclaimer.
// 
// 2. Redistributions in binary form must reproduce the above copyright
//    notice, this list of conditions and the following disclaimer in
//    the documentation and/or other materials provided with
//    the distribution.
// 
// 3. Neither the names of the copyrighters, the name of the project
//    which is related to this software (hereinafter referred to as
//    "project") nor the names of the contributors may be used to
//    endorse or promote products derived from this software without
//    specific prior written permission.
// 
// 4. No merchantable use may be permitted without prior written
//    notification to the copyrighters.
// 
// 5. The copyrighters, the project and the contributors may prohibit
//    the use of this software at any time.
// 
// THIS SOFTWARE IS PROVIDED BY THE COPYRIGHTERS, THE PROJECT AND
// CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING
// BUT NOT LIMITED THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS
// FOR A PARTICULAR PURPOSE, ARE DISCLAIMED.  IN NO EVENT SHALL THE
// COPYRIGHTERS, THE PROJECT OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT,
// INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
// (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
// SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
// HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT,
// STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING
// IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
// POSSIBILITY OF SUCH DAMAGE.
//
// $Id: sendUcastNS2.def,v 1.1.1.1 2000/10/31 22:39:35 sekiya Exp $

#include "nd.def"

//----------------------------------------------------------------------
// echo-request
//	TN(link-local) ==> NUT(link-local)
//----------------------------------------------------------------------
FEM_icmp6_echo_request(echo_request, _HETHER_tn2nut,
	{
	 _SRC(tnv6());
	 _DST(nutv6());},
	{
	 payload=echo_data;
	}
)

//----------------------------------------------------------------------
// echo-reply
//	NUT(link-local) ==> TN(link-local)
//----------------------------------------------------------------------
FEM_icmp6_echo_reply(echo_reply, _HETHER_nut2tn,
	{
	 _SRC(nutv6());
	 _DST(tnv6());
	},
	{
	 payload=echo_data;
	}
)

//----------------------------------------------------------------------
Payload echo_data {
	data=repeat(0x11,10);
}

//----------------------------------------------------------------------
// unicast NA
//	TN(link-local) ==> NUT(link-local)
//	target=TN(link-local)
//	r=0, s=1, o=1
//	w/ TLLA
//----------------------------------------------------------------------
FEM_icmp6_na(na, _HETHER_tn2nut,
	{
	 _SRC(tnv6());
	 _DST(nutv6());
	 HopLimit=255;
	},
	{
	 RFlag=0;
	 SFlag=1;
	 OFlag=1;
	 TargetAddress=tnv6();
	 option=_TLLOPT_tn;
	}
)

//----------------------------------------------------------------------
// multicast NS
//	NUT(link-local) ==> TN(solicited-node[link-local])
//	target=TN(link-local)
//	w/ SLLA
//----------------------------------------------------------------------
FEM_icmp6_ns(multicast_ns, _HETHER_nut2tnsolnode,
	{
	 _SRC(nutv6());
	 _DST(_IPV6_SOLNODE_MCAST(tnv6()));
	 HopLimit=255;
	},
	{
	 TargetAddress=tnv6();
	 option=_SLLOPT_nut;
	}
)

//----------------------------------------------------------------------
// unicast NS
//	NUT(link-local) ==> TN(link-local)
//	target=TN(link-local)
//----------------------------------------------------------------------
FEM_icmp6_ns(unicast_ns, _HETHER_nut2tn,
	{
	 _SRC(nutv6());
	 _DST(tnv6());
	 HopLimit=255;
	},
	{
	 TargetAddress=tnv6();
	}
)

//----------------------------------------------------------------------
// unicast NS
//	NUT(link-local) ==> TN(link-local)
//	target=TN(link-local)
//----------------------------------------------------------------------
FEM_icmp6_ns(unicast_ns_sll, _HETHER_nut2tn,
	{
	 _SRC(nutv6());
	 _DST(tnv6());
	 HopLimit=255;
	},
	{
	 TargetAddress=tnv6();
	 option=_SLLOPT_nut;
	}
)

//----------------------------------------------------------------------
_HETHER_define(hether_x2allnode, ether(A0N_MAC_ADDR),
	v62ethermulti(v6(_ALLNODES_MCAST_ADDR)))
_SLLOPT_define(sllopt_x, ether(A0N_MAC_ADDR))

//----------------------------------------------------------------------
// multicast RA
//	X(link-local) ==> all-node
//	m=0, o=0
//	lifetime=600, reachableTime=0, *retransTimer=3000
//----------------------------------------------------------------------
FEM_icmp6_ra(unsol_ra_set, hether_x2allnode,
	{
	 _SRC(v6ether(A0N_MAC_ADDR));
	 _DST(v6(_ALLNODES_MCAST_ADDR));
	 HopLimit=255;
	},
	{
	 CurHopLimit=0;
	 MFlag=0;
	 OFlag=0;
	 LifeTime=600;
	 ReachableTime=0;
	 RetransTimer=3000;
         option=sllopt_x;
	}
)

//----------------------------------------------------------------------
// multicast RA
//	X(link-local) ==> all-node
//	m=0, o=0
//	lifetime=600, reachableTime=0, *retransTimer=1000
//----------------------------------------------------------------------
FEM_icmp6_ra(unsol_ra_clrtimer, hether_x2allnode,
	{
	 _SRC(v6ether(A0N_MAC_ADDR));
	 _DST(v6(_ALLNODES_MCAST_ADDR));
	 HopLimit=255;
	},
	{
	 CurHopLimit=0;
	 MFlag=0;
	 OFlag=0;
	 LifeTime=600;
	 ReachableTime=0;
	 RetransTimer=1000;
	}
)

//----------------------------------------------------------------------
// multicast RA
//	X(link-local) ==> all-node
//	m=0, o=0
//	*lifetime=0, reachableTime=0, retransTimer=0
//----------------------------------------------------------------------
FEM_icmp6_ra(unsol_ra_clrrtr, hether_x2allnode,
	{
	 _SRC(v6ether(A0N_MAC_ADDR));
	 _DST(v6(_ALLNODES_MCAST_ADDR));
	 HopLimit=255;
	},
	{
	 CurHopLimit=0;
	 MFlag=0;
	 OFlag=0;
	 LifeTime=0;
	 ReachableTime=0;
	 RetransTimer=0;
	}
)

//----------------------------------------------------------------------
