//
// $Copyright$
//
// $Name:  $
//
// $Id: HTR_E_common.def,v 1.1.1.1 2000/10/31 22:38:51 sekiya Exp $
//

#ifndef IPSEC_ECHO_DATA
#define IPSEC_ECHO_DATA echo_data
#endif

#include "./HTR_common.def"

//======================================================================

Payload echo_data {
	data = {
		0x50, 0x61, 0x64, 0x4c, 0x65, 0x6e, 0x20, 0x69,
		0x73, 0x20, 0x5a, 0x65, 0x72, 0x6f
	};
}

Payload echo_data_odd {
	data = { 0x4f, 0x64, 0x64, 0x44, 0x61, 0x74, 0x61};
}

//======================================================================
//
// Algorithm predefinition
//

ESPAlgorithm ealgo_descbc_012 {
	crypt = descbc("01234567");
}

ESPAlgorithm ealgo_descbc_foo {
	crypt = descbc("foo0foo1");
}

ESPAlgorithm ealgo_descbc_012_hmacmd5_012 {
	crypt = descbc("01234567");
	auth = hmacmd5("0123456789ABCDEF");
}

ESPAlgorithm ealgo_descbc_012_hmacmd5_foo {
	crypt = descbc("01234567");
	auth = hmacmd5("foo0foo1foo2foo3");
}

ESPAlgorithm ealgo_descbc_012_hmacsha1_012 {
	crypt = descbc("01234567");
	auth = hmacsha1("0123456789ABCDEF0123");
}

ESPAlgorithm ealgo_descbc_012_hmacsha1_foo {
	crypt = descbc("01234567");
	auth = hmacsha1("foo0foo1foo2foo3foo4");
}

ESPAlgorithm ealgo_null {
	crypt = null_crypt(4);
}

ESPAlgorithm ealgo_null_hmacmd5_012 {
	crypt = null_crypt(4);
	auth = hmacmd5("0123456789ABCDEF");
}

ESPAlgorithm ealgo_null_hmacsha1_012 {
	crypt = null_crypt(4);
	auth = hmacsha1("0123456789ABCDEF0123");
}

ESPAlgorithm ealgo_3descbc_012 {
	crypt = des3cbc("0123456789ABCDEFGHIJKLMN");
}

ESPAlgorithm ealgo_3descbc_012_hmacmd5_012 {
	crypt = des3cbc("0123456789ABCDEFGHIJKLMN");
	auth = hmacmd5("0123456789ABCDEF");
}

ESPAlgorithm ealgo_3descbc_012_hmacsha1_012 {
	crypt = des3cbc("0123456789ABCDEFGHIJKLMN");
	auth = hmacsha1("0123456789ABCDEF0123");
}

//======================================================================
//
// ESP definition (default use)
//

#ifndef EALGO_FROM_HOST1
#define EALGO_FROM_HOST1 ealgo_descbc_012
#endif

Hdr_ESP esp_from_host {
	SPI = 0x1000;
	SequenceNumber = 1;
	algorithm = EALGO_FROM_HOST1;
}

#ifndef EALGO_TO_HOST1
#define EALGO_TO_HOST1 ealgo_descbc_012
#endif

Hdr_ESP esp_to_host {
	SPI = 0x1000;
	SequenceNumber = any;	// 1;
	algorithm = EALGO_TO_HOST1;
}

//======================================================================
//
// Echo Request from Host1 IPsec ESP
//

#ifndef ESP_FROM_HOST1
#define ESP_FROM_HOST1 esp_from_host
#endif

FEM_icmpX_echo_request_exth(
	echo_request_from_host1_esp,
	hether_router2nut,
	{
		_SRC(vX(IPSEC_HOST1_NET5_ADDR));
		_DST(vX(IPSEC_NUT_NET3_ADDR));
	},
	{
		header = _HDR_IPVX_NAME(echo_request_from_host1_esp);
		exthdr = ESP_FROM_HOST1;
		upper = _ICMPVX_NAME(echo_request_from_host1_esp);
	},
	{
		payload = IPSEC_ECHO_DATA;
	}
)

//======================================================================
//
// Echo Reply to Host1 IPsec ESP
//

#ifndef ESP_TO_HOST1
#define ESP_TO_HOST1 esp_to_host
#endif

FEM_icmpX_echo_reply_exth(
	echo_reply_to_host1_esp,
	hether_nut2router,
	{
		_SRC(vX(IPSEC_NUT_NET3_ADDR));
		_DST(vX(IPSEC_HOST1_NET5_ADDR));
	},
	{
		header = _HDR_IPVX_NAME(echo_reply_to_host1_esp);
		exthdr = ESP_TO_HOST1;
		upper = _ICMPVX_NAME(echo_reply_to_host1_esp);
	},
	{
		payload = IPSEC_ECHO_DATA;
	}
)

