//
// Copyright (C) 1999,2000 Yokogawa Electric Corporation and
//                         YDC Corporation.
// All rights reserved.
// 
// Redistribution and use of this software in source and binary
// forms, with or without modification, are permitted provided that
// the following conditions and disclaimer are agreed and accepted
// by the user:
// 
// 1. Redistributions of source code must retain the above copyright
//    notice, this list of conditions and the following disclaimer.
// 
// 2. Redistributions in binary form must reproduce the above copyright
//    notice, this list of conditions and the following disclaimer in
//    the documentation and/or other materials provided with
//    the distribution.
// 
// 3. Neither the names of the copyrighters, the name of the project
//    which is related to this software (hereinafter referred to as
//    "project") nor the names of the contributors may be used to
//    endorse or promote products derived from this software without
//    specific prior written permission.
// 
// 4. No merchantable use may be permitted without prior written
//    notification to the copyrighters.
// 
// 5. The copyrighters, the project and the contributors may prohibit
//    the use of this software at any time.
// 
// THIS SOFTWARE IS PROVIDED BY THE COPYRIGHTERS, THE PROJECT AND
// CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING
// BUT NOT LIMITED THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS
// FOR A PARTICULAR PURPOSE, ARE DISCLAIMED.  IN NO EVENT SHALL THE
// COPYRIGHTERS, THE PROJECT OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT,
// INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
// (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
// SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
// HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT,
// STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING
// IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
// POSSIBILITY OF SUCH DAMAGE.
//
// $Name:  $
//
// $Id: IH_Router.def,v 1.1.1.1 2000/10/31 22:39:52 sekiya Exp $
//

#define TN_GL0_ADDR tn2v6(_GLOBAL0_UCAST_PRFX,_GLOBAL0_UCAST_PRFXLEN,"Link0")
#define TN_GL1_ADDR tn2v6(_GLOBAL1_UCAST_PRFX,_GLOBAL1_UCAST_PRFXLEN,"Link1")
#define NUT_GL0_ADDR nut2v6(_GLOBAL0_UCAST_PRFX,_GLOBAL0_UCAST_PRFXLEN,"Link0")
#define NUT_GL1_ADDR nut2v6(_GLOBAL1_UCAST_PRFX,_GLOBAL1_UCAST_PRFXLEN,"Link1")

#define PING_ID	0xffff
#define PING_SN	0x0001

#ifndef TRAFFIC_CLASS
#define TRAFFIC_CLASS	0
#endif
#ifndef FLOW_LABEL
#define FLOW_LABEL	0
#endif
#ifndef HOP_LIMIT
#define HOP_LIMIT	64
#endif


//======================================================================
//
// ICMP echo request
//

FEM_icmp6_echo_request(
	echo_request_to_link0,
	_HETHER_tn2nut,
	{
		TrafficClass = TRAFFIC_CLASS;
		FlowLabel = FLOW_LABEL;
		HopLimit = HOP_LIMIT;
		_SRC(TN_GL0_ADDR);
		_DST(TN_GL1_ADDR);
	},
	{
		Identifier = PING_ID;
		SequenceNumber = PING_SN;
		payload = echo_data8;
	}
)


FEM_icmp6_echo_request(
	echo_request_from_link1,
	_HETHER_nut2tn,
	{
		TrafficClass = TRAFFIC_CLASS;
		FlowLabel = FLOW_LABEL;
		_SRC(TN_GL0_ADDR);
		_DST(TN_GL1_ADDR);
	},
	{
		Identifier = PING_ID;
		SequenceNumber = PING_SN;
		payload = echo_data8;
	}
)

//======================================================================
//
// ICMP echo reply
//

FEM_icmp6_echo_reply(
	echo_reply_to_link1,
	_HETHER_tn2nut,
	{
		TrafficClass = TRAFFIC_CLASS;
		FlowLabel = FLOW_LABEL;
		HopLimit = HOP_LIMIT;
		_SRC(TN_GL1_ADDR);
		_DST(TN_GL0_ADDR);
	},
	{
		Identifier = PING_ID;
		SequenceNumber = PING_SN;
		payload = echo_data8;
	}
)


FEM_icmp6_echo_reply(
	echo_reply_from_link0,
	_HETHER_nut2tn,
	{
		TrafficClass = TRAFFIC_CLASS;
		FlowLabel = FLOW_LABEL;
		_SRC(TN_GL1_ADDR);
		_DST(TN_GL0_ADDR);
	},
	{
		Identifier = PING_ID;
		SequenceNumber = PING_SN;
		payload = echo_data8;
	}
)

//----------------------------------------------------------------------
// Payload Data
//----------------------------------------------------------------------

Payload echo_data8 {
	data = {1,2,3,4,5,6,7,8};
}

//======================================================================
//
// NS and NA for Link0 (Link Local)
//

FEM_icmp6_ns(
	ns_from_link0_ll,
	_HETHER_nut2tnsolnode,
	{
		_SRC(nutv6());
		_DST(_IPV6_SOLNODE_MCAST(tnv6()));
		HopLimit = 255;
	},
	{
		TargetAddress = TN_GL0_ADDR;
		option = _SLLOPT_nut;
	}
)

FEM_icmp6_na(
	na_to_link0_ll,
	_HETHER_tn2nut,
	{
		_SRC(tnv6());
		_DST(nutv6());
		HopLimit = 255;
	},
	{
		SFlag = 1;
		OFlag = 1;
		TargetAddress = TN_GL0_ADDR;
		option = _TLLOPT_tn;
	}
)

//======================================================================
//
// NS and NA for Link0 (Global)
//

FEM_icmp6_ns(
	ns_from_link0,
	_HETHER_nut2tnsolnode,
	{
		_SRC(NUT_GL0_ADDR);
		_DST(_IPV6_SOLNODE_MCAST(tnv6()));
		HopLimit = 255;
	},
	{
		TargetAddress = TN_GL0_ADDR;
		option = _SLLOPT_nut;
	}
)

FEM_icmp6_na(
	na_to_link0,
	_HETHER_tn2nut,
	{
		_SRC(tnv6());
		_DST(NUT_GL0_ADDR);
		HopLimit = 255;
	},
	{
		SFlag = 1;
		OFlag = 1;
		TargetAddress = TN_GL0_ADDR;
		option = _TLLOPT_tn;
	}
)

//======================================================================
//
// NS and NA for Link1 (Link Local)
//

FEM_icmp6_ns(
	ns_from_link1_ll,
	_HETHER_nut2tnsolnode,
	{
		_SRC(nutv6());
		_DST(_IPV6_SOLNODE_MCAST(tnv6()));
		HopLimit = 255;
	},
	{
		TargetAddress = TN_GL1_ADDR;
		option = _SLLOPT_nut;
	}
)

FEM_icmp6_na(
	na_to_link1_ll,
	_HETHER_tn2nut,
	{
		_SRC(tnv6());
		_DST(nutv6());
		HopLimit = 255;
	},
	{
		SFlag = 1;
		OFlag = 1;
		TargetAddress = TN_GL1_ADDR;
		option = _TLLOPT_tn;
	}
)

//======================================================================
//
// NS and NA for Link1 (Global)
//

FEM_icmp6_ns(
	ns_from_link1,
	_HETHER_nut2tnsolnode,
	{
		_SRC(NUT_GL1_ADDR);
		_DST(_IPV6_SOLNODE_MCAST(tnv6()));
		HopLimit = 255;
	},
	{
		TargetAddress = TN_GL1_ADDR;
		option = _SLLOPT_nut;
	}
)

FEM_icmp6_na(
	na_to_link1,
	_HETHER_tn2nut,
	{
		_SRC(tnv6());
		_DST(NUT_GL1_ADDR);
		HopLimit = 255;
	},
	{
		SFlag = 1;
		OFlag = 1;
		TargetAddress = TN_GL1_ADDR;
		option = _TLLOPT_tn;
	}
)
